For 1990-2009 cars

### Removal

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Disconnect the intake air temperature (IAT) sensor.
3. Remove the air cleaner outlet hose from the throttle body.
4. Remove the breather tube from the camshaft cover.
5. Remove the air cleaner housing bolts.
6. Remove the air cleaner housing.

### Installation

1. Install the air cleaner housing.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the air cleaner housing bolts.

Tighten
Tighten the air cleaner housing bolts to 10 N·m (89 lb in).

3. Connect the air intake tube to the throttle body.
4. Connect the breather tube to the valve cover.
5. Connect the IAT sensor.
6. Connect the negative battery cable.