For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Air Deflector Screws | 2 N·m | 18 lb in
Chime Module Screws | 4 N·m | 35 lb in
Clock Screws | 2 N·m | 18 lb in
Cupholder Screws | 2.5 N·m | 22 lb in
Deposit Box Screws | 2.5 N·m | 22 lb in
Driver Knee Bolster Bolts | 10 N·m | 89 lb in
Floor Console Brace Bolts | 4 N·m | 35 lb in
Floor Console Brace Nuts | 4 N·m | 35 lb in
HVAC Controls Screws | 4 N·m | 35 lb in
Instrument Cluster Screws | 4 N·m | 35 lb in
Instrument Cluster Trim Panel Screws | 4 N·m | 35 lb in
Instrument Panel Bolts Behind the HVAC Controls | 4 N·m | 35 lb in
Instrument Panel End Bolts | 20 N·m | 15 lb ft
Instrument Panel End Screws | 4 N·m | 35 lb in
Instrument Panel Nuts Above the Steering Column | 20 N·m | 15 lb ft
Steering Column Bracket Nut | 22 N·m | 16 lb ft
Steering Column Lower Trim Cover Screws | 2.5 N·m | 22 lb in
Steering Column U-Clamp Nuts | 22 N·m | 16 lb ft
Steering Column Upper Trim Cover Screws | 3 N·m | 27 lb in