For 1990-2009 cars

## Fascia Grille Replacement Five Door

### Removal Procedure

1. Open the hood.
2. Remove the screws.
3. Using a flat-bladed tool, disconnect the clips.
4. Remove the fascia grille.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

Install the radiator grille with the screws.

## Fascia Grille Replacement Four Door/Wagon

### Removal Procedure

1. Open the hood.
2. Remove the screws and the radiator grille.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

Install the radiator grille with the screws.