For 1990-2009 cars

## Refrigerant Tubes Replacement Diesel Engine

### Removal Procedure

Note: The Left-Hand Drive is Shown. The Right-Hand Drive is Similiar

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Recover the refrigerant. Refer to Refrigerant Recovery and Recharging.
3. Remove the nut at the discharge hose block connected to the compressor.
4. Remove the headlamp housing at the left-hand side. Refer to Headlamp Replacement.
5. Remove the nut at the condenser connecting block.
6. Remove the refrigerant discharge hose.
7. Remove the air cleaner housing bolts and the air filter housing assembly.
8. Disconnect the electrical connector at the pressure transducer.
9. Remove the liquid pipe block-to-expansion valve retaining nut at the fire wall.
10. Remove the headlamp housing at the right-hand side. Refer to Headlamp Replacement.
11. Remove the liquid pipe block-to-receiver dryer retaining nut.
12. Remove the bolts which secure the support clamps that hold the liquid pipe to the vehicle.
13. Remove the liquid pipe from the vehicle.
14. Cap the opening at the receiver-dryer to prevent contamination.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Position the liquid pipe into the vehicle.
2. Install the liquid pipe support clamp bolts and tighten to 8 N·m (71 lb in).
3. Install a new O-ring on the pipe at the receiver dryer.
4. Install the liquid pipe block-to-receiver-dryer retaining nut and tighten to 14 N·m (10 lb ft).
5. Install the headlamp housing at the right-hand side. Refer to Headlamp Replacement.
6. Install the liquid evaporator pipe block retaining nut to the fire wall and tighten to 14 N·m (10 lb ft).
7. Connect the electrical connector at the pressure transducer.
8. Install the air cleaner housing bolts and the air filter housing assembly.
9. Position the refrigerant discharge hose into the vehicle.
10. Install the nut at the condenser connecting block and tighten to 16 N·m (12 lb ft).
11. Install the headlamp housing at the left-hand side. Refer Headlamp Replacement.
12. Install the nut at the discharge hose block connected to the compressor and tighten to 33 N·m (24 lb ft).
13. Connect the negative battery cable.
14. Evacuate and recharge the A/C system. Refer to Refrigerant Recovery and Recharging.

## Refrigerant Tubes Replacement Gasoline Engine

### Removal Procedure

Note: The Left-Hand Drive is Shown. The Right-Hand Drive is Similiar

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Recover the refrigerant. Refer to Refrigerant Recovery and Recharging.
3. Remove the nut at the discharge hose block connected to the compressor.
4. Remove the headlamp housing at the left-hand side. Refer to Headlamp Replacement.
5. Remove the nut at the condenser connecting block.
6. Remove the refrigerant discharge hose.
7. Remove the air cleaner housing bolts and the air filter housing assembly.
8. Disconnect the electrical connector at the pressure transducer.
9. Remove the liquid pipe block-to-expansion valve retaining nut at the fire wall.
10. Remove the headlamp housing at the right-hand side. Refer to Headlamp Replacement.
11. Remove the liquid pipe block-to-receiver dryer retaining nut.
12. Remove the bolts which secure the support clamps that hold the liquid pipe to the vehicle.
13. Remove the liquid pipe from the vehicle.
14. Cap the opening at the receiver-dryer to prevent contamination.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Position the liquid pipe into the vehicle.
2. Install the liquid pipe support clamp bolts and tighten to 8 N·m (71 lb in).
3. Install a new O-ring on the pipe at the receiver dryer.
4. Install the liquid pipe block-to-receiver-dryer retaining nut and tighten to 14 N·m (10 lb ft).
5. Install the headlamp housing at the right-hand side. Refer to Headlamp Replacement.
6. Install the liquid evaporator pipe block retaining nut to the fire wall and tighten to 14 N·m (10 lb ft).
7. Connect the electrical connector at the pressure transducer.
8. Install the air cleaner housing bolts and the air filter housing assembly.
9. Position the refrigerant discharge hose into the vehicle.
10. Install the nut at the condenser connecting block and tighten to 16 N·m (12 lb ft).
11. Install the headlamp housing at the left-hand side. Refer Headlamp Replacement.
12. Install the nut at the discharge hose block connected to the compressor and tighten to 33 N·m (24 lb ft).
13. Connect the negative battery cable.
14. Evacuate and recharge the A/C system. Refer to Refrigerant Recovery and Recharging.