For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Air Cleaner Housing Bolts | 10 N·m | 89 lb in
Camshaft Cap Bolts | 16 N·m | 12 lb ft
Camshaft Cover Nuts | 10 N·m | 89 lb in
Connecting Rod Bearing Cap Bolts | 25 N·m +30°+15° | 18 lb ft +30°+15°
Coolant Temperature Sensor | 20 N·m | 15 lb ft
Crankshaft Bearing Cap Bolts | 50 N·m +45°+15° | 37 lb ft +45°+15°
Crankshaft Cover Nuts | 5-8 N·m | 44-71 lb in
Crankshaft Pulley Bolt | 95 N·m +30°+15° | 70 lb ft +30°+15°
Cylinder Head Bolts -- Cylinder Head Mounting Bolts | 25+70° +70°+50° | 18+70° +70°+50°
Direct Ignition System Coil Mounting Bolts | 10 N·m | 89 lb in
Direct Ignition System Coil Mounting Bracket Bolts | 10 N·m | 89 lb in
Engine Mount Attaching Bolts | 30 N·m | 22 lb ft
Engine Mount Bracket Attaching Bolts/Nuts | 50 N·m | 37 lb ft
Exhaust Camshaft Gear Bolt | 67.5 N·m | 49 lb ft
Exhaust Flex Pipe-to-Catalytic Converter or Connecting Pipe Retaining Nut | 35 N·m | 26 lb ft
Exhaust Flex Pipe-to-Exhaust Manifold Retaining Nuts | 35 N·m | 26 lb ft
Exhaust Gas Recirculation Valve Adapter Bolts | 25 N·m | 18 lb ft
Exhaust Manifold Heat Shield Bolts | 15 N·m | 11 lb ft
Exhaust Manifold Retaining Nuts | 25 N·m | 18 lb ft
Flexible Plate Bolts | 60 N·m | 44 lb ft
Flexible Plate Inspection Cover Bolts | 10 N·m | 89 lb in
Flywheel Bolts | 35 N·m +30°+15° | 25 lb ft +30°+15°
Flywheel Inspection Cover Bolts | 12 N·m | 106 lb in
Front Timing Belt Cover Bolts -- Upper and Lower | 10 N·m | 89 lb in
Fuel Rail Assembly Retaining Bolts | 25 N·m | 18 lb ft
Fuel Rail Retaining Bolts | 25 N·m | 18 lb ft
Generator Upper Retaining Bolt | 20 N·m | 15 lb ft
Intake Camshaft Gear Bolt | 67.5 N·m | 49 lb ft
Intake Manifold Retaining Bolts/Nuts | 25 N·m | 18 lb ft
Intake Manifold Support Bracket Lower Bolt | 25 N·m | 18 lb ft
Intake Manifold Support Bracket Upper Bolts | 25 N·m | 18 lb ft
Lower Front Timing Belt Cover Bolts | 10 N·m | 89 lb in
Oil Pan Drain Plug | 35 N·m | 26 lb ft
Oil Pan Flange Bolts | 75 N·m | 55 lb ft
Oil Pan Retaining Bolts | 10 N·m | 89 lb in
Oil Pressure Switch | 40 N·m | 30 lb ft
Oil Pump Bolts | 10 N·m | 89 lb in
Oil Pump Rear Cover Bolts | 8 N·m | 71 lb in
Oil Pump Retaining Bolts | 10 N·m | 89 lb in
Oil Suction Pipe or Support Bracket Bolts | 10 N·m | 89 lb in
Rear Timing Belt Cover Bolts | 10 N·m | 89 lb in
Safety Relief Valve Bolt | 30 N·m | 22 lb ft
Spark Plugs | 25 N·m | 18 lb ft
Thermostat Housing Mounting Bolts | 20 N·m | 15 lb ft
Timing Belt Automatic Tensioner Bolts | 25 N·m | 18 lb ft
Timing Belt Idler Pulley Bolt | 40 N·m | 30 lb ft
Transaxle Bell Housing Bolts | 75 N·m | 55 lb ft
Transaxle Torque Converter Bolts | 45 N·m | 33 lb ft
Upper Front Timing Belt Cover Bolts | 10 N·m | 89 lb in
Water Pump Retaining Bolts | 10 N·m | 89 lb in