For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the tire and wheel assembly. Refer to Tire and Wheel Removal and Installation .
3. Remove the tire from the wheel. Refer to Tire Dismounting and Mounting .
4. Remove the tire pressure sensor from the valve using a TORX driver.
5. Remove the valve.

### Installation Procedure

1. Apply soapy water to the surface of the valve for easy fitting.
2. Install the valve and the tire pressure sensor to the wheel.
3. Ensure the valve and the tire pressure sensor are seated properly.
4. Install the tire to the wheel. Refer to Tire Dismounting and Mounting .
5. Install the tire and wheel assembly. Refer to Tire and Wheel Removal and Installation .
6. Lower the vehicle.