For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the bolts and the front fog lamp.
3. Disconnect the electrical connector.
4. Remove the fog lamp access cover.
5. Remove the retaining wire.
6. Remove the bulb.

### Installation Procedure

1. Install the bulb.
2. Install the retaining wire.
3. Install the fog lamp access cover.
4. Connect the electrical connector.

Notice: Refer to Fastener Notice in the Preface section.

5. Install the front fog lamp with the bolts.

Tighten
Tighten the front fog lamp bolts to 4 N·m (35 lb in).

6. Connect the negative battery cable.