For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.

Caution: Refer to Vehicle Lifting Caution in the Preface section.

2. Raise and suitably support the vehicle.
3. Disconnect the rear wheel speed sensor electrical connector.
4. Remove the rear hub unit from the knuckle assembly. Refer to Rear Wheel Bearing and Hub Replacement .

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the rear hub unit to the knuckle assembly. Refer to Rear Wheel Bearing and Hub Replacement .
2. Connect the rear wheel speed sensor electrical connector.
3. Connect the negative battery cable.