For 1990-2009 cars

## Cargo Area Rear Trim Panel Replacement Sedan

#### Tools Required

J 21104-B Weatherstrip Remover Universal

### Removal Procedure

1. Remove the luggage compartment rear panel cover. Refer to Rear Compartment Trim Panel Replacement .
2. Remove the plastic retaining clips using the J 21104-B and reposition the luggage compartment rear trim panel.

### Installation Procedure

1. Install the wheelhouse trim panel with the plastic clips.
2. Install the luggage compartment rear panel cover. Refer to Rear Compartment Trim Panel Replacement .

## Cargo Area Rear Trim Panel Replacement Liftgate

#### Tools Required

J 21104-B Weatherstrip Remover Universal

### Removal Procedure

1. Remove the rear compartment trim panel. Refer to Rear Compartment Trim Panel Replacement .
2. Remove the cargo area rear trim panel plastic retaining clips (1) using the J 21104-B .
3. Remove the cargo area rear trim panel retaining screw.

### Installation Procedure

1. Position the cargo area rear trim panel.
2. Install the cargo area rear trim panel retaining screw.
3. Install the rear cargo area trim panel plastic clips (1).
4. Install the rear compartment trim panel. Refer to Rear Compartment Trim Panel Replacement .