For 1990-2009 cars

### Removal Procedure

1. Remove the plastic cap to reveal the lower center pillar seat belt anchor.
2. Remove the bolt and the lower center pillar seat belt anchor.
3. Remove the lower center pillar trim panel. Refer to Center Pillar Lower Trim Panel Replacement .
4. Remove the plastic cap to reveal the upper center pillar seat belt anchor.
5. Remove the bolt and the upper center pillar seat belt anchor.
6. Remove the screws from the seat belt retractor bracket.
7. Remove the bolt and the seat belt retractor.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the seat belt retractor with the bolt.

Tighten
Tighten the seat belt retractor bolt to 38 N·m (28 lb ft).

2. Install the seat belt retractor bracket with the screw.

Tighten
Tighten the seat belt bracket screw to 3 N·m (27 lb in).

3. Install the upper center pillar seat belt anchor with the bolt.

Tighten
Tighten the seat belt anchor bolt to 38 N·m (28 lb ft).

4. Install the seat belt anchor plastic cap.
5. Install the lower center pillar trim panel. Refer to Center Pillar Lower Trim Panel Replacement .
6. Install the lower center pillar seat belt anchor with the bolt.

Tighten
Tighten the seat belt anchor bolt to 38 N·m (28 lb ft).

7. Install the seat belt anchor plastic cap.