For 1990-2009 cars

Checks | Actions
--- | ---
Inspect for an out-of-valance tire or wheel. | Balance the tire or the wheel.
Inspect for excessive wheel hub runout. | Measure the hub flange runout. Replace the hub as needed.
Inspect for excessive brake drum or brake rotor imbalance. | Adjust the brakes. Replace the brake rotor or the brake drum as needed.
Inspect for worn tie rod ends. | Replace the outer tie rods.
Inspect for wheel trim imbalance. | Balance the wheel.
Inspect for a worn lower ball joint. | Replace the lower ball joint.
Inspect for excessive wheel runout. | Measure the wheel runout. Replace the wheel as needed.
Inspect for excessive loaded radial runout on the tire and wheel assembly | Match-mount the tire and wheel assembly.