For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the manifold absolute pressure (MAP) sensor electrical connector.
3. Disconnect the MAP sensor vacuum hose.
4. Remove the MAP sensor bolt.
5. Remove the MAP sensor.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the MAP sensor with the bolt.

Tighten
Tighten the MAP sensor bolt to 8 N·m (71 lb in).

2. Connect the MAP sensor vacuum hose.
3. Connect the MAP sensor electrical connector.
4. Connect the negative battery cable.