For 1990-2009 cars

#### Tools Required

J 22912-B Split-Plate Bearing Puller

1. Using a hydraulic press and J 22912-B under the gear, install a new front bearing on the countershaft.

1.1. | Install the bearing collar race on the countershaft.

1.2. | Install the bearing assembly with the retaining ring groove forward.

1.3. | Install the bearing inner race using a suitable press tube.

Important: The retaining ring is a select fit. Always install a new retaining ring.

2. Select the maximum thickness retaining ring for the countershaft front bearing, that will fit in the groove. Refer to Countershaft Front Bearing Retaining Ring Specifications .
3. Install the countershaft front bearing retaining ring.