For 1990-2009 cars

### Removal Procedure

1. Separate the retaining strips on the shift lever boot.
2. Lift upward on the shift lever bezel to release the retaining tabs.
3. Lift the bezel and boot over the shift lever.
4. If necessary, remove the boot assembly from the bezel by releasing the wire retainer and position locator (1).

### Installation Procedure

1. If necessary, install the boot to the bezel ensuring the position locator (1) is pointing forward.
2. Lower the bezel and boot over the shift lever.
3. Ensure the retaining tabs are properly indexed to the console.
4. Push downward on the shift lever bezel to seat the retaining tabs.
5. Attach the retaining strips on the shift lever boot.