For 1990-2009 cars

#### Special Tools

• | J 25025-1 Dial Indicator Mounting Post

• | J 36850 Transjel Lubricant

• | J 39855 Stator Shaft Seal Installer

1. Install the J 25025-1 .
2. Remove the J 39855-2 which is part of kit J 39855 .
3. Install the pump to drum thrust washer (601).
4. Use J 36850 or equivalent to retain the washer to the pump.
5. Install the pump cover to case gasket (6).

Important: The oil pump to case seal is installed after the oil pump assembly, during torque converter installation. Refer to Converter Housing Installation .

6. Install the oil pump assembly (4) into the case and align all holes properly.

Notice: Refer to Fastener Notice in the Preface section.

Important: The pump to case bolt O-ring seals (3) must be replaced.

7. Install the pump to case bolts (2) with new O-ring seals (3).

Tighten
Tighten the bolts to 29 N·m (21 lb ft).

8. Remove the J 25025-1 .
9. Install the remaining pump to case bolts (2) and O-ring seals (3), in the holes where the J 25025-1 were.

Tighten
Tighten the bolts to 29 N·m (21 lb ft).