For 1990-2009 cars

### Removal Procedure

1. Release the park brake.
2. Raise the vehicle. Refer to Lifting and Jacking the Vehicle .
3. Remove the wheel house inner liner. Refer to Front Wheelhouse Liner Replacement .
4. Remove the park brake cable adjusting nut.
5. Remove the front park brake cable from the equalizer.
6. Remove the retaining bolt for the front park brake cable.
7. Remove the knee bolster panel. Refer to Knee Bolster Replacement .
8. Remove the clutch pedal assembly. Refer to Clutch Pedal Replacement .
9. Remove the electrical connector from the brake switch.
10. Remove the park brake cable pedal mounting bolts.
11. Remove the front park brake cable weather seal.
12. Remove the park brake pedal assembly from the vehicle.
13. Remove the front park brake pedal and cable assembly from the vehicle noting routing for installation.

### Installation Procedure

1. Install the park brake pedal and cable assembly as previously routed.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the mounting bolts for the park brake pedal assembly.

Tighten
Tighten the park brake pedal mounting bolts to 20 N·m (15 lb ft).

3. Install the front park brake cable weather seal.
4. Install the clutch pedal assembly. Refer to Clutch Pedal Replacement .
5. Install the retaining bolt for the front park brake cable at the wheel well.

Tighten
Tighten the front park brake retaining bolt to 20 N·m (15 lb ft).

6. Install the front park brake cable to the equalizer.
7. Install the park brake cable adjusting nut. Refer to Park Brake Adjustment .
8. Install the wheel house liner. Refer to Front Wheelhouse Liner Replacement .
9. Install the knee bolster panel. Refer to Knee Bolster Replacement .
10. Lower the vehicle.