For 1990-2009 cars

## Engine Flywheel Cleaning and Inspection Automatic Transmission

1. Inspect the engine flywheel for cracks (1).
2. Inspect the engine flywheel teeth for damage (2).
3. Replace the engine flywheel if damage is present.

## Engine Flywheel Cleaning and Inspection Manual Transmission

Important: In order to maintain the proper component balance, contact surface taper and heat transfer, manual transmission flywheels are NOT to be machined.

1. Inspect the engine flywheel for damaged teeth (1).
2. Inspect the engine flywheel for cracks, hot spots, or any surface damage (2).
3. Replace the engine flywheel if damage is present.