For 1990-2009 cars

### Removal Procedure

1. Remove the power steering pump from the vehicle, if necessary. Refer to Power Steering Pump Replacement .

Important: Protect the drive shaft with the shim stock.

2. Use a small chisel in order to remove the seal.

Discard the seal.

### Installation Procedure

1. Lubricate the new drive shaft seal using power steering fluid.
2. Use a deep socket in order to install the new drive shaft seal.
3. Install the power steering pump, if removed. Refer to Power Steering Pump Replacement .