For 1990-2009 cars

## Engine Flywheel Installation Automatic Transmission

#### Special Tools

J 45059 Angle Meter

For equivalent regional tools, refer to Special Tools.

1. Install the flywheel.

Caution: Refer to Fastener Caution in the Preface section.

2. Install new flywheel bolts.

2.1. | Tighten the new flywheel bolts to 40 N·m (30 lb ft).

2.2. | Use J 45059 meter to tighten the flywheel bolts an additional 45 degrees.

## Engine Flywheel Installation Manual Transmission

#### Special Tools

J 45059 Angle Meter

For equivalent regional tools, refer to Special Tools.

1. Install the flywheel.

Caution: Refer to Fastener Caution in the Preface section.

2. Install new flywheel bolts.

2.1. | Tighten the new flywheel bolts to 40 N·m (30 lb ft).

2.2. | Use J 45059 meter to tighten the flywheel bolts an additional 45 degrees.