For 1990-2009 cars

### Removal Procedure

1. Remove the screw securing the jack cover to the jack stowage bracket.
2. Remove the jack cover by lifting up to release the tab from behind the jack stowage bracket.

### Installation Procedure

1. Position the jack cover over the jack stowage bracket ensuring that the tab on the rear of the cover hooks behind the top of the jack stowage bracket.
2. Install the screw securing the jack cover to the jack stowage bracket.

Tighten
Tighten the jack cover screw until fully seated, tight, but not stripped.