For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel (I/P) storage compartment assembly. Refer to Instrument Panel Storage Compartment Replacement.
2. Remove the screws retaining the storage compartment back panel.
3. Remove the back panel from the storage compartment.

### Installation Procedure

1. Install the back panel to the storage compartment.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the screws retaining the storage compartment back panel. Tighten the screws to 3 N·m (27 lb in).
3. Install the instrument panel (I/P) storage compartment assembly. Refer to Instrument Panel Storage Compartment Replacement.