For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel (I/P) assembly. Refer to Instrument Panel Assembly Replacement.
2. Remove the air distributor duct (1) from the instrument panel.

### Installation Procedure

1. Install the air distributor duct (1) to the instrument panel.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the retaining screws to the air distributor duct. Tighten the screws to 1.9 N·m (17 lb in).
3. Install the I/P assembly. Refer to Instrument Panel Assembly Replacement.