For 1990-2009 cars

#### Special Tools

J 35582 Oil Pump Seal Installer

### Removal Procedure

1. Remove the rear propeller shaft. Refer to One-Piece Propeller Shaft Replacement.

Caution: Refer to Transfer Case Seal Removal Caution in the Preface section.

2. Using a flat-bladed screwdriver and a hammer, remove the rear output shaft seal from the transfer case.

### Installation Procedure

1. Using the J 35582 and a hammer, install the rear output shaft seal into the transfer case.
2. Install the rear propeller shaft. Refer to One-Piece Propeller Shaft Replacement.
3. Inspect the transfer case fluid level. Refer to Transfer Case Fluid Replacement.