For 1990-2009 cars

## Radiator Outlet Hose Replacement LLV, LLR

#### Tools Required

J 38185 Hose Clamp Pliers

### Removal Procedure

1. Drain the coolant. Refer to Cooling System Draining and Filling .
2. Using J 38185 reposition the outlet radiator hose clamp away from the thermostat housing (1).
3. Remove the outlet radiator hose from the thermostat.
4. Raise the vehicle. Refer to Lifting and Jacking the Vehicle .
5. Using J 38185 reposition the outlet radiator hose clamp away from the radiator.
6. Remove the outlet radiator hose (1) from the radiator.

### Installation Procedure

1. Install the outlet radiator hose (1) to the radiator.
2. Using J 38185 reposition the outlet radiator hose clamp to the radiator.
3. Lower the vehicle.
4. Install the outlet radiator hose to the thermostat (1).
5. Using J 38185 reposition the outlet radiator hose clamp to the thermostat housing.
6. Fill the cooling system. Refer to Cooling System Draining and Filling .

## Radiator Outlet Hose Replacement LH8

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Drain the cooling system. Refer to Cooling System Draining and Filling .
2. Remove the air cleaner assembly. Refer to Air Cleaner Assembly Replacement .
3. Use J 38185 to release the radiator hose clamps.
4. Release hose from retainer on fan shroud.

1 | Radiator Outlet Hose Clamp (Qty: 2).
2 | Radiator Outlet Hose.