For 1990-2009 cars

### Removal Procedure

1. Raise the hood. Support the hood with something other than the prop rod.
2. Remove the bolt retaining the prop rod to the radiator support.
3. Remove the prop rod.

### Installation Procedure

1. Install the prop rod to the radiator support.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the prop rod bolt and tighten to 10 N·m (89 lb in).
3. Remove the temporary hood support.