For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Disable the supplemental inflatable restraint (SIR) system. Refer to SIR Disabling and Enabling .
2. Disconnect the battery negative cable. Refer to Battery Negative Cable Disconnection and Connection .
3. Remove the lower steering column trim cover. Refer to Steering Column Trim Covers Replacement .

1 | Ignition/Start Switch Electrical Connector
2 | Ignition/Start Switch Bolt (Qty: 2) Notice: Refer to Fastener Notice in the Preface section. Tighten 0.74 N·m (7 lb in)
3 | Ignition/Start Switch

#### Procedure

Turn the ignition lock cylinder to the run position prior to removing the ignition/start switch.