For 1990-2009 cars

#### Special Tools

• | EN 46547 Flywheel Holding Tool

• | EN-48034 Harmonic Balancer Installer

• | J 41816-A Crankshaft Balancer Remover

• | J 41816-2 Crankshaft End Protector

• | J 45059 Angle Meter

### Removal Procedure

1. Remove the radiator. Refer to Radiator Replacement.
2. Remove the drive belt. Refer to Drive Belt Replacement.
3. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
4. Remove the service slot plug.

Important: The crankshaft balancer does not have a key-way; so the crankshaft could turn when tightening, causing an improper torque.

5. Install the EN 46547 (1) into the flywheel teeth.
6. Lower the vehicle.
7. Remove and discard the crankshaft balancer bolt.
8. Install the J 41816-2 and J 41816-A to the crankshaft balancer.

Important: Do not pull on outer edge of the crankshaft balancer.

9. Remove the crankshaft balancer.
10. Remove the J 41816-2 and J 41816-A .

### Installation Procedure

1. Install the crankshaft balancer using the EN-48034 .
2. Remove the EN-48034 .

Notice: Refer to Fastener Notice in the Preface section.

3. Install the crankshaft balancer washer and NEW bolt.

Tighten
Tighten the bolt to 150 N·m (111 lb ft) plus an additional 180 degrees using the J 45059 .

4. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
5. Remove the EN 46547 (1) from the flywheel teeth.
6. Install the service slot plug.
7. Lower the vehicle.
8. Install the drive belt. Refer to Drive Belt Replacement.
9. Install the radiator. Refer to Radiator Replacement.