For 1990-2009 cars

### Removal Procedure

1. Raise the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove engine protection shield. Refer to Engine Protection Shield Replacement
3. Disconnect the transmission fluid cooler lines (3) from the radiator. Refer to Transmission Fluid Cooler Hose/Pipe Quick-Connect Fitting Disconnection and Connection.
4. Remove the transmission fluid cooler lines from the retainer located on the radiator.
5. Remove the transmission fluid cooler lines from the retainer located on the right side of the engine.
6. Support the transmission with a transmission jack.
7. Remove the transmission support. Refer to Transmission Support Crossmember Replacement.
8. Remove the front exhaust pipe assembly. Refer to Catalytic Converter Replacement.
9. Carefully lower the transmission to gain access to the transmission fluid cooler line fittings.
10. Disconnect the transmission fluid cooler lines (2) from the transmission. Refer to Transmission Fluid Cooler Hose/Pipe Quick-Connect Fitting Disconnection and Connection.
11. Remove the transmission fluid cooler lines (1) from the vehicle.

### Installation Procedure

Caution: Ensure that the cooler line being installed has a plastic cap on each end that connects to a quick connect fitting. If no plastic cap exists, or the plastic cap is damaged, obtain a new plastic cap and position on to the cooler line prior to the cooler line installation.

1. Install the transmission fluid cooler lines (1) to the vehicle.
2. Install the transmission fluid cooler lines (2) to the transmission. Refer to Transmission Fluid Cooler Hose/Pipe Quick-Connect Fitting Disconnection and Connection.
3. Raise the transmission into position.
4. Install the front exhaust pipe assembly. Refer to Catalytic Converter Replacement.
5. Install the transmission support. Refer to Transmission Support Crossmember Replacement.
6. Remove the transmission jack.
7. Install the clip that holds the transmission fluid cooler lines together.
8. Install the transmission fluid cooler lines to the right side of the engine.
9. Install the transmission fluid cooler line to the retainer located on the radiator.
10. Install the transmission fluid cooler lines (3) to the radiator. Refer to Transmission Fluid Cooler Hose/Pipe Quick-Connect Fitting Disconnection and Connection.
11. Install engine protection shield. Refer to Engine Protection Shield Replacement
12. Lower the vehicle.
13. Fill the transmission to the proper level with DEXRON® VI transmission fluid. Refer to Transmission Fluid Check.