For 1990-2009 cars

### Removal Procedure

1. Remove the seat back recliner handle. Refer to Driver or Passenger Seat Recliner Handle Replacement.
2. Remove the 3 screws retaining the trim panel to the seat.
3. Remove the front seat cushion outer trim panel from the vehicle.

### Installation Procedure

1. Align the front seat cushion outer trim panel to the seat assembly.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the 3 seat cushion outer trim panel mounting screws.

Tighten
Tighten the front seat cushion outer trim panel screws to 1.5 N·m (13 lb in).

3. Install the seat back recliner handle. Refer to Driver or Passenger Seat Recliner Handle Replacement.