For 1990-2009 cars

### Removal Procedure

Important: Do not allow the wiper arm (1) to fall back and strike the windshield.

1. Lift the wiper arm and hold in the upright position.
2. Push upward the locking tab (3) of the wiper blade clip and pull downward on the wiper arm blade (2).
3. Remove the wiper blade from the inside radius of the wiper arm.
4. Bring the wiper arm out through the opening in the wiper blade.

### Installation Procedure

1. Position the wiper blade in the inside radius of the wiper arm hook.
2. Insert the hook of the wiper arm through the opening in the wiper blade (2).
3. Pull upward until the locking tab (3) of the pivot engages the slot in the hook.
4. Carefully lower the wiper arm and blade onto the windshield.