For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Place a suitable drain pan under the oil filter.
3. Remove the oil filter (437).
4. Remove the oil filter adapter (438).

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the oil filter adapter (438).

Tighten
Tighten the adapter to 55 N·m (40 lb ft).

2. Lubricate the oil filter seal with clean engine oil.
3. Install the oil filter (437).

Tighten
Tighten the filter to 30 N·m (22 lb ft).

4. Lower the vehicle.
5. Refill the engine oil. Refer to Approximate Fluid Capacities and/or Fluid and Lubricant Recommendations.
6. Start the engine and inspect for leaks.