For 1990-2009 cars

### Removal Procedure

1. Remove the grille. Refer to Grille Replacement .
2. Remove the fog lamps, if applicable. Refer to Front Fog Lamp Replacement .
3. Remove the bolts that attach the bumper bracket to the frame.
4. Remove the bumper from the vehicle.
5. Remove the bolts that attach the bumper bracket to the bumper.
6. Remove the front bumper fascia (2) from the bumper (1). Refer to Front Bumper Fascia Replacement .

### Installation Procedure

1. Install the front bumper fascia (2) to the bumper (1). Refer to Front Bumper Fascia Replacement .
2. Install the bumper bracket to the bumper.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the bumper to bracket bolts.

Tighten
Tighten the bolts to 40 N·m (30 lb ft).

4. Install the bumper to the vehicle.
5. Install the bumper bracket to frame bolts.

Tighten
Tighten the bolts to 40 N·m (30 lb ft).

6. Install the fog lamps, if applicable. Refer to Front Fog Lamp Replacement .
7. Install the grille. Refer to Grille Replacement .