For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Accessory Drive Belt Idler Pulley Bolt | 50 N·m | 37 lb ft
Accessory Drive Belt Tensioner Bolts | 50 N·m | 37 lb ft
Automatic Transmission Flex Plate Bolts - First Pass | 20 N·m | 15 lb ft
Automatic Transmission Flex Plate Bolts - Second Pass | 50 N·m | 37 lb ft
Automatic Transmission Flex Plate Bolts - Final Pass | 100 N·m | 74 lb ft
Battery Cable Channel Bolt | 12 N·m | 106 lb in
Camshaft Position (CMP) Sensor Bolt | 12 N·m | 106 lb in
Camshaft Position (CMP) Sensor Wire Harness Bolt | 12 N·m | 106 lb ft
Camshaft Retainer Bolts - Hex Head Bolts | 25 N·m | 18 lb ft
Camshaft Retainer Bolts - TORX Head Bolts | 15 N·m | 11 lb ft
Camshaft Sprocket Bolt - First Pass | 75 N·m | 55 lb ft
Camshaft Sprocket Bolt - Final Pass | 50 degrees
Connecting Rod Bolts - First Pass | 20 N·m | 15 lb ft
Connecting Rod Bolts - Final Pass | 85 degrees
Coolant Air Bleed Pipe and Cover Bolts | 12 N·m | 106 lb in
Coolant Temperature Sensor | 20 N·m | 15 lb ft
Crankshaft Balancer Bolt - First Pass | 150 N·m | 111 lb ft
Crankshaft Balancer Bolt - Second Pass | Loosen 360 degrees
Crankshaft Balancer Bolt - Third Pass | 50 N·m | 37 lb ft
Crankshaft Balancer Bolt - Final Pass | 230 degrees
Crankshaft Bearing Cap M8 Bolts | 25 N·m | 18 lb ft
Crankshaft Bearing Cap M10 Bolts - First Pass in Sequence | 20 N·m | 15 lb ft
Crankshaft Bearing Cap M10 Bolts - Final Pass in Sequence | 80 degrees
Crankshaft Bearing Cap M10 Studs - First Pass in Sequence | 20 N·m | 15 lb ft
Crankshaft Bearing Cap M10 Studs - Final Pass in Sequence | 51 degrees
Crankshaft Oil Deflector Nuts | 25 N·m | 18 lb ft
Crankshaft Position (CKP) Sensor Bolt | 25 N·m | 18 lb ft
Crankshaft Rear Oil Seal Housing Bolts | 30 N·m | 22 lb ft
Cylinder Head M8 Bolts - in Sequence | 30 N·m | 22 lb ft
Cylinder Head M11 Bolts - First Pass in Sequence | 30 N·m | 22 lb ft
Cylinder Head M11 Bolts - Second Pass in Sequence | 90 degrees
Cylinder Head M11 Bolts - Final Pass in Sequence | 70 degrees
Cylinder Head Plug | 20 N·m | 15 lb ft
Engine Block Coolant Drain Hole Plug | 60 N·m | 44 lb ft
Engine Block Coolant Heater | 50 N·m | 37 lb ft
Engine Block Oil Gallery Plugs | 60 N·m | 44 lb ft
Engine Harness Ground Strap Bolt/Stud | 16 N·m | 12 lb ft
Engine Harness-to-Generator Bracket Bolt | 9 N·m | 80 lb in
Engine Harness Retainer-to-Intake Manifold Nut | 5 N·m | 44 lb in
Engine Mount Bracket Through Bolt | 100 N·m | 74 lb ft
Engine Mount-to-Engine Block Bolts | 55 N·m | 41 lb ft
Evaporative (EVAP) Emission Pipe Bracket Nut | 20 N·m | 15 lb ft
Exhaust Manifold Bolts - First Pass | 15 N·m | 11 lb ft
Exhaust Manifold Bolts - Final Pass | 20 N·m | 15 lb ft
Exhaust Manifold Heat Shield Bolts | 9 N·m | 80 lb in
Exhaust Manifold Studs | 20 N·m | 15 lb ft
Front Cover Bolts | 25 N·m | 18 lb ft
Fuel Injection Fuel Rail Bolts | 10 N·m | 89 lb in
Fuel Injection Fuel Rail Crossover Tube Bolts | 3.8 N·m | 34 lb in
Fuel Rail Stop Bracket Bolt | 50 N·m | 37 lb ft
Generator Bracket Bolts | 50 N·m | 37 lb ft
Ignition Coil Bracket-to-Valve Rocker Arm Cover Studs | 12 N·m | 106 lb in
Ignition Coil-to-Bracket Bolts | 10 N·m | 89 lb in
Intake Manifold Bolts - First Pass in Sequence | 5 N·m | 44 lb in
Intake Manifold Bolts - Final Pass in Sequence | 10 N·m | 89 lb in
Intake Manifold Sight Shield Retainer Bolts | 5 N·m | 44 lb in
J 41798 M8 Bolt | 25 N·m | 18 lb ft
J 41798 M10 Bolts | 50 N·m | 37 lb ft
Knock Sensor Bolts | 25 N·m | 18 lb ft
Negative Battery Cable Stud | 25 N·m | 18 lb ft
Oil Filter | 30 N·m | 22 lb ft
Oil Filter Fitting | 55 N·m | 40 lb ft
Oil Level Indicator Switch | 13 N·m | 115 lb in
Oil Level Indicator Tube Bolt | 25 N·m | 18 lb ft
Oil Pan Baffle Bolts | 9 N·m | 80 lb in
Oil Pan Closeout Cover Bolt - Left Side | 9 N·m | 80 lb in
Oil Pan Closeout Cover Bolt - Right Side | 9 N·m | 80 lb in
Oil Pan Cover Bolts | 9 N·m | 80 lb in
Oil Pan Drain Plug | 25 N·m | 18 lb ft
Oil Pan M6 Bolts - Oil Pan-to-Rear Housing | 12 N·m | 106 lb in
Oil Pan M8 Bolts - Oil Pan-to-Engine Block and Oil Pan-to-Front Cover | 25 N·m | 18 lb ft
Oil Pressure Relief Valve | 27 N·m | 20 lb ft
Oil Pressure Sensor | 35 N·m | 26 lb ft
Oil Pump Cover Bolts | 12 N·m | 106 lb in
Oil Pump Relief Valve Plug | 12 N·m | 106 lb in
Oil Pump Screen Nuts | 25 N·m | 18 lb ft
Oil Pump Screen-to-Oil Pump Bolts | 12 N·m | 106 lb in
Oil Pump-to-Engine Block Bolts | 25 N·m | 18 lb ft
Power Steering Pump-to-Engine Block Bolts | 50 N·m | 37 lb ft
Spark Plugs | 15 N·m | 11 lb ft
Throttle Body Bolts | 10 N·m | 89 lb in
Throttle Body Nuts | 10 N·m | 89 lb in
Throttle Body Studs | 6 N·m | 53 lb in
Timing Chain Tensioner Bolts | 25 N·m | 18 lb ft
Valley Cover Bolts | 25 N·m | 18 lb ft
Valve Lifter Guide Bolts | 12 N·m | 106 lb in
Valve Rocker Arm Bolts | 30 N·m | 22 lb ft
Valve Rocker Arm Cover Bolts | 12 N·m | 106 lb in
Water Inlet Housing Bolts | 15 N·m | 11 lb ft
Water Pump Bolts - First Pass | 15 N·m | 11 lb ft
Water Pump Bolts - Final Pass | 30 N·m | 22 lb ft