For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
1 | Check for worn or damaged outer wheel drive shaft joints and/or seals. Are the outer wheel drive shaft joints/seals worn? | Go to Step 2 | System OK
2 | Check for proper clearance between the wheel drive shaft and other components. Correct as necessary. Is the repair complete? | System OK | Go to Step 3
3 | Replace the outer CV joints/seals. Refer to Wheel Drive Shaft Outer Joint and Boot Replacement . Is the repair complete? | System OK | --