For 1990-2009 cars

## Locking Differential Clutch Disc Assembly Disassemble 8.0 Inch Axle

1. Remove the guide clips (2).
2. Remove the clutch discs and the splined discs (3 - 7) from the side gear (1).

## Locking Differential Clutch Disc Assembly Disassemble 8.6 Inch Axle

1. Remove the guide clips (3).
2. Remove the clutch discs and the splined discs (2, 4-6) from the locking differential side gear (1).