For 1990-2009 cars

## Transmission Mount Replacement 2WD

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Support the transmission with a transmission jack.
3. Remove the 2 nuts securing the transmission mount to the transmission support.
4. Raise the transmission off of the transmission support.
5. Remove the transmission mount bolts (4).
6. Remove the transmission mount (3).
7. Remove the transmission mount spacer bolts (1).
8. Remove the transmission mount spacer (2).

### Installation Procedure

1. Install the transmission mount spacer (2).
2. Install the transmission mount spacer bolts (1).
3. Install the transmission mount (3).

Notice: Refer to Fastener Notice in the Preface section.

4. Install the bolts (4).

Tighten
Tighten the bolts to 55 N·m (41 lb ft).

5. Lower the transmission and install the 2 nuts securing the transmission mount to the transmission support.

Tighten
Tighten the nuts to 57 N·m (42 lb ft).

6. Remove the transmission jack.
7. Lower the vehicle.

## Transmission Mount Replacement 4WD

### Removal Procedure

1. Remove the transmission support. Refer to Transmission Support Crossmember Replacement .
2. Remove the transmission mount bolts.
3. Remove the transmission mount from the vehicle.

### Installation Procedure

1. Install the transmission mount to the vehicle.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the bolts.

Tighten
Tighten the bolts to 55 N·m (41 lb ft).

3. Install the transmission support. Refer to Transmission Support Crossmember Replacement .