For 1990-2009 cars

### Removal Procedure

Caution: Refer to SIR Caution in the Preface section.

1. Disable the supplemental inflatable restraint (SIR) system. Refer to SIR Disabling and Enabling .
2. Disengage the shift lever seal (2) from the steering column trim covers (1) and slide it up the shift lever (4).
3. Remove the shift lever bolt (3) from the shift lever (4).
4. Remove the shift lever with the shift lever seal from the steering column.
5. Transfer any parts as needed.

### Installation Procedure

1. Install the shift lever with the shift lever seal to the steering column.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the shift lever bolt (3).

Tighten
Tighten the bolt to 20 N·m (15 lb ft).

3. Align and secure the shift lever seal (2) to the steering column trim covers (1).
4. Enable the SIR system. Refer to SIR Disabling and Enabling .