For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Support the rear axle at curb height.
3. Remove the stabilizer shaft insulator bracket mounting bolts.
4. Remove the stabilizer shaft insulator brackets.
5. Remove the stabilizer shaft insulators.

### Installation Procedure

1. Install the stabilizer shaft insulators to the stabilizer shaft.
2. Install the stabilizer shaft insulator brackets to the rear axle.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the stabilizer shaft bracket mounting bolts and tighten to 50 N·m (37 lb ft).
4. Remove the rear axle support.
5. Lower the vehicle.