For 1990-2009 cars

#### Special Tools

• | J 8092 Driver Handle

• | J 23062-14 Bushing Remover

• | J 34196-B Transmission Bushing Service Set

1. Inspect the case extension for the following conditions:

• | Porosity

• | Cracks

• | Nicks

• | Burrs

• | Worn bushings

2. Remove the case extension oil seal assembly (34) (model dependent).
3. Using the J 23062-14 and the J 8092 , remove the case extension bushing (33).
4. Using the J 34196-4 which is part of kit J 34196-B and the J 8092 , install a case extension bushing (33).