For 1990-2009 cars

### Removal Procedure

1. Open the front and side access doors.
2. Remove the rear door outer auxiliary weatherstrip by pulling the weatherstrip from the rear door pinchweld flange.

### Installation Procedure

1. Install the rear door auxiliary weatherstrip to the rear door pinchweld flange, by pressing the weatherstrip into place until it is fully seated.
2. Close the front and side doors.