For 1990-2009 cars

#### Tools Required

J 44219 Engine Cover Alignment Pins

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

1. Install the engine front cover spacer bolt.

Tighten
Tighten the engine front cover spacer bolt to 10 N·m (89 lb in).

2. Install J 44219 .
3. Remove 2 bolts from the engine front cover in the location of the alignment pins.

Important: The engine front cover must be installed within 10 minutes from when the sealer was applied.

4. Apply a 3 mm (0.12 in) bead of sealer GM P/N 12378521 (Canadian P/N 88901148) to the block sealing surface (1).
5. Align the oil pump to the crankshaft sprocket splines.
6. Install the engine front cover and bolts.
7. Remove J 44219 .
8. Install the 2 remaining engine front cover bolts.

Tighten

1. Tighten the engine front cover bolts to 10 N·m (89 lb in).
2. Tighten the small center bolt (1) last to 8 N·m (71 lb in).