For 1990-2009 cars

## Endgate Emblem/Nameplate Replacement Colorado LS

Callout | Component Name
--- | ---
1 | Endgate Nameplate/Emblem (Colorado LS) Notice: Refer to Exterior Trim Emblem Removal Notice in the Preface section.

#### Procedure

1. Use a J 25070 or equivalent to remove the old nameplate. Clean all the adhesive residue from the endgate, wipe the surface dry with a clean lint-free towel prior to installing new nameplate.
2. When removing protective liners from adhesive backed nameplates, be careful not to touch the tape with hands and do not allow the tape to come in contact with dirt or any foreign matter prior to adhesion.
3. Close the endgate prior to installing the new nameplate/emblem to the endgate.
4. Remove the protective liner from the back side of the adhesive tape.
5. Align the nameplate/emblem to the endgate and press to ensure full adhesion is made.

## Endgate Emblem/Nameplate Replacement Colorado

Callout | Component Name
--- | ---
1 | Endgate Nameplate/Emblem (Colorado) Notice: Refer to Exterior Trim Emblem Removal Notice in the Preface section.

#### Procedure

1. Use a J 25070 or equivalent to remove the old nameplate. Clean all the adhesive residue from the endgate, wipe the surface dry with a clean lint-free towel prior to installing new nameplate.
2. When removing protective liners from adhesive backed nameplates, be careful not to touch the tape with hands and do not allow the tape to come in contact with dirt or any foreign matter prior to adhesion.
3. Close the endgate prior to installing the new nameplate/emblem to the endgate.
4. Remove the protective liner from the back side of the adhesive tape.
5. Align the nameplate/emblem to the endgate and press to ensure full adhesion is made.

## Endgate Emblem/Nameplate Replacement GMC SLE

Callout | Component Name
--- | ---
1 | Endgate Nameplate/Emblem (Canyon SLE) Notice: Refer to Exterior Trim Emblem Removal Notice in the Preface section.

#### Procedure

1. Use a J 25070 or equivalent to remove the old nameplate. Clean all the adhesive residue from the endgate, wipe the surface dry with a clean lint-free towel prior to installing new nameplate.
2. When removing protective liners from adhesive backed nameplates, be careful not to touch the tape with hands and do not allow the tape to come in contact with dirt or any foreign matter prior to adhesion.
3. Close the endgate prior to installing the new nameplate/emblem to the endgate.
4. Remove the protective liner from the back side of the adhesive tape.
5. Align the nameplate/emblem to the endgate and press to ensure full adhesion is made.

## Endgate Emblem/Nameplate Replacement GMC Canyon SL

Callout | Component Name
--- | ---
1 | Endgate Nameplate/Emblem (Canyon SL) Notice: Refer to Exterior Trim Emblem Removal Notice in the Preface section.

#### Procedure

1. Use a J 25070 or equivalent to remove the old nameplate. Clean all the adhesive residue from the endgate, wipe the surface dry with a clean lint-free towel prior to installing new nameplate.
2. When removing protective liners from adhesive backed nameplates, be careful not to touch the tape with hands and do not allow the tape to come in contact with dirt or any foreign matter prior to adhesion.
3. Close the endgate prior to installing the new nameplate/emblem to the endgate.
4. Remove the protective liner from the back side of the adhesive tape.
5. Align the nameplate/emblem to the endgate and press to ensure full adhesion is made.

2 | Endgate Nameplate/Emblem (GMC) Notice: Refer to Exterior Trim Emblem Removal Notice in the Preface section.

#### Procedure

1. Use a J 25070 or equivalent to remove the old nameplate/emblem. Clean all the adhesive residue from the endgate, wipe the surface dry with a clean lint-free towel prior to installing new nameplate.
2. When removing protective liners from adhesive backed nameplates/emblems, be careful not to touch the tape with hands and do not allow the tape to come in contact with dirt or any foreign matter prior to adhesion.
3. Close the endgate prior to installing the new nameplate/emblem to the endgate.
4. Remove the protective liner from the back side of the adhesive tape.
5. Align the nameplate/emblem to the endgate and press to ensure full adhesion is made.

## Endgate Emblem/Nameplate Replacement Colorado LT

Callout | Component Name
--- | ---
1 | Endgate Nameplate/Emblem (Colorado) Notice: Refer to Exterior Trim Emblem Removal Notice in the Preface section.

#### Procedure

1. Use a J 25070 or equivalent to remove the old nameplate. Clean all the adhesive residue from the endgate, wipe the surface dry with a clean lint-free towel prior to installing new nameplate.
2. When removing protective liners from adhesive backed nameplates, be careful not to touch the tape with hands and do not allow the tape to come in contact with dirt or any foreign matter prior to adhesion.
3. Close the endgate prior to installing the new nameplate/emblem to the endgate.
4. Remove the protective liner from the back side of the adhesive tape.
5. Align the nameplate/emblem to the endgate and press to ensure full adhesion is made.

## Endgate Emblem/Nameplate Replacement ISUZU i290

Callout | Component Name
--- | ---
1 | Endgate Nameplate/Emblem (ISUZU) Notice: Refer to Exterior Trim Emblem Removal Notice in the Preface section.

#### Procedure

1. Use a J 25070 or equivalent to remove the old nameplate. Clean all the adhesive residue from the endgate, wipe the surface dry with a clean lint-free towel prior to installing new nameplate.
2. When removing protective liners from adhesive backed nameplates, be careful not to touch the tape with hands and do not allow the tape to come in contact with dirt or any foreign matter prior to adhesion.
3. Close the endgate prior to installing the new nameplate/emblem to the endgate.
4. Remove the protective liner from the back side of the adhesive tape.
5. Align the nameplate/emblem to the endgate and press to ensure full adhesion is made.

2 | Endgate Emblem Decal (i-290) Notice: Refer to Exterior Trim Emblem Removal Notice in the Preface section.

#### Procedure

1. Use a J 25070 or equivalent to remove the old decal. Clean all the adhesive residue from the endgate, wipe the surface dry with a clean lint-free towel prior to installing new decal.
2. When removing protective liners from adhesive backed decals, be careful not to touch the tape with hands and do not allow the tape to come in contact with dirt or any foreign matter prior to adhesion.
3. Close the endgate prior to installing the new decal to the endgate.
4. Remove the protective liner from the back side of the decal.
5. Align the decal to the endgate and press to ensure full adhesion is made.