For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Lower the headliner trim panel to access the antenna base fastener. Refer to Headlining Trim Panel Replacement.

1 | Digital Radio and Mobile Telephone and Vehicle Location Base Assembly Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

1. Loosen the integral nut.
2. Disconnect the electrical connections.
3. Disconnect the antenna cables.
4. Feed the wiring and cable up through the hole in the roof panel.

Tighten
10 N·m (89 lb in)