For 1990-2009 cars

### Removal Procedure

1. Remove the accessory drive belt. Refer to Drive Belt Replacement - Accessory.
2. Loosen the drive belt idler pulley bolt and remove the idler pulley.

### Installation Procedure

1. Position the drive belt idler pulley to the generator bracket and tighten the idler pulley bolt finger tight.

Caution: Refer to Fastener Caution in the Preface section.

2. Tighten the drive belt idler pulley bolt.

Tighten
Tighten the bolt to 50 N·m (37 lb ft).

3. Install the accessory drive belt. Refer to Drive Belt Replacement - Accessory.