For 1990-2009 cars

## Coolant Heater Replacement LLV,LLR

### Removal Procedure

1. Raise and support the vehicle only high enough to access the coolant heater (6) through the wheelhouse. Refer to Lifting and Jacking the Vehicle .
2. Remove the left wheelhouse liner. Refer to Front Wheelhouse Liner Replacement .
3. Disconnect the coolant heater cord (4) from the coolant heater (6).
4. Remove the coolant heater from the engine block.

### Installation Procedure

1. Locate the block heater hole on side of block.
2. While lining up the retaining clip on the block heater to notch on block, insert the block heater and snap into place.
3. Connect the coolant heater cord (4) to the coolant heater (6).
4. Install the left wheelhouse liner. Refer to Front Wheelhouse Liner Replacement .
5. Lower the vehicle.