For 1990-2009 cars

### Removal Procedure

Warning: Refer to Brake Dust Warning in the Preface section.

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle
2. Remove the tire and wheel assembly. Refer to Tire and Wheel Removal and Installation.
3. Remove the wheel hub and bearing assembly. Refer to Front Wheel Bearing and Hub Replacement.
4. Remove the front brake shield.
5. Remove any debris or corrosion from the front brake shield, wheel hub and steering knuckle mating surfaces.

### Installation Procedure

1. Install the front brake shield.
2. Install the wheel hub and bearing assembly. Refer to Front Wheel Bearing and Hub Replacement.
3. Install the tire and wheel assembly. Refer to Tire and Wheel Removal and Installation.