For 1990-2009 cars

Checks | Action
--- | ---
DEFINITION: Knocking or clunking noise occurs when operating the vehicle in high gear or coasting in neutral at 16 km/h (10 mph).
One or more of the universal joints are worn or damaged. | Replace the universal joint. Refer to Universal Joint Replacement - External Snap Ring .
The side gear hub counterbore in the differential is worn oversize. | Replace the differential case and/or the side gears. Refer to Differential Replacement .