For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the rear wheel speed sensor. Refer to Rear Wheel Speed Sensor Replacement.
3. Remove the park brake cable from the rear brake backing plate. Refer to Parking Brake Rear Cable Replacement - Left Side or Parking Brake Rear Cable Replacement - Right Side.
4. Remove the wheel cylinder. Refer to Wheel Cylinder Replacement.
5. Remove the rear axle shaft. Refer to Rear Axle Shaft Replacement.
6. Remove the rear brake backing plate bolts (1).
7. Remove the rear brake backing plate (1).

### Installation Procedure

1. Install the rear brake backing plate (1).

Caution: Refer to Fastener Caution in the Preface section.

2. Install the rear brake backing plate bolts (1) and tighten to 135 N·m (100 lb ft).
3. Install the rear axle shaft. Refer to Rear Axle Shaft Replacement.
4. Install the wheel cylinder. Refer to Wheel Cylinder Replacement.
5. Install the park brake cable to the rear brake backing plate. Refer to Parking Brake Rear Cable Replacement - Left Side or Parking Brake Rear Cable Replacement - Right Side.
6. Install the rear wheel speed sensor. Refer to Rear Wheel Speed Sensor Replacement.