For 1990-2009 cars

## Engine Flywheel Replacement with Automatic Transmission

#### Special Tools

J 45059 Angle Meter

### Removal Procedure

1. Remove the transmission. Refer to Transmission Replacement .
2. Remove and discard the flywheel bolts.
3. Remove the flywheel.

### Installation Procedure

1. Position the flywheel to the crankshaft

Notice: Refer to Fastener Notice in the Preface section.

2. Install the new flywheel bolts.

Tighten
Tighten the flywheel bolts to 40 N·m (30 lb ft) plus an additional 45 degrees using the J 45059 .

3. Install the transmission. Refer to Transmission Replacement .

## Engine Flywheel Replacement with Manual Transmission

#### Special Tools

J 45059 Angle Meter

### Removal Procedure

1. Remove the clutch assembly. Refer to Clutch Assembly Replacement .
2. Remove and discard the flywheel bolts.
3. Remove the flywheel.

### Installation Procedure

1. Position the flywheel to the crankshaft

Notice: Refer to Fastener Notice in the Preface section.

2. Install the new flywheel bolts.

Tighten
Tighten the flywheel bolts to 40 N·m (30 lb ft) plus an additional 45 degrees using the J 45059 .

3. Install the clutch assembly. Refer to Clutch Assembly Replacement .