For 1990-2009 cars

### Removal Procedure

1. Place the transmission in neutral.
2. Release the park brake, if applied.
3. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
4. Mark the rear universal joint to the drive shaft flange.
5. Remove the retaining bolts and clamps.
6. Remove the propeller shaft from the pinion drive flange.
7. Remove the propeller shaft from the transmission/transfer case.
8. Using tape or a rubber band, wrap the U-Joint bearing caps to ensure the bearing caps do not separate from the U-Joint.

### Installation Procedure

1. Remove the tape or rubber band from the U-Joint.
2. Install the propeller shaft in the transmission/transfer case.
3. Align the propeller shaft with the reference marks on the pinion flange.

Caution: Refer to Fastener Caution in the Preface section.

4. Install the clamps and retaining bolts and tighten the bolts to 20 N·m (15 lb ft).
5. Lower the vehicle.